## Please enable JavaScript to view this site.

# MDaemon Email Server 26.0

- Zoom Window Out
- Larger Text | Smaller Text
- Hide Page Header
- Show Expanding Text
- Printable Version
- Save Permalink URL

Binding | Scroll Prev Top Next More

Outbound Binding Settings

Enable outbound IP binding

When this option is checked, MDaemon always binds outbound sockets. For domains that have This domain recognizes only connections made to these IPs checked on the Host Name & IP screen, MDaemon uses the domain's configured IP. Otherwise it uses the Default address(es) for outbound socket binding specified below.

Default address(es) for outbound socket binding: IPv4/IPv6 address

These are the IP addresses that will be used for outbound socket binding for domains that are not already bound to specific IP addresses on the Domain Manager's Host Name & IP screen.

Inbound Binding Settings

Second IP address for inbound socket binding: IPv4/IPv6 address

Use this option if you wish to designate a second set of IP addresses for inbound socket binding.

See:

Domain Manager » Host Name & IP

IPv6

MDaemon v26.0.1 - April 2026. Copyright © 1996-2026. All rights reserved. MDaemon Technologies